Assembly Hints

Significant points remembered from previous gazebo erections!

	•	Assemble top frame first, noting the alpha numeric designations for the poles.  
	•	When inserting the vertical poles (two steps) make sure to have 4 people helping, one for each corner.
	•	Canopy should be laid on top of frame before last (bottom) half of vertical poles are inserted.  This allows for easier centering of canopy over top frame.
	•	Do not forget to attach the hooks at the bottom of each corner of the canopy to one of the three holes at the lower end of each bottom vertical pole.
	•	Before securing the small vertical pole footing bases to the ground with pegs, zip the screening closed so feet will not be located too far apart to allow later screen closing.
	•	Once in place, tie down gazebos with tent pegs and adjustable nylon strings that should be in each gazebo case.

Dave K2YG

Disassembly 

Should be done in orderly fashion with inventory taken carefully. One year parts were all jumbled by zealous helpers.